Turn this control connection to a data connection.
The data connection stays open until it is deleted
using the delh command, or the control connection
specified by the parameter to the data command is
closed.
